BlitB3Saw BLIT derived sawtooth

BlitB3Saw.ar(freq, leak, mul, add )

Band limited impulse generator based on B-Spline interpolation of order 3, integrated to create a sawtooth waveform.

freq Maximum frequency is a period of 4 samples, so a quarter of the sampling rate. You may start to hear aliasing over 5000 Hz or so, otherwise perceptually indistinguishable from an analog waveform.

leak leaky coefficient. 0 would give back the impulses, higher numbers (up to near 1.0) fill out the inter-impulse space, integrating the waveform.

See also: BlitB3, BlitB3Square, BlitB3Tri

{ BlitB3Saw.ar(XLine.kr(1000, 20, 10)) }.play;

//aliasing suddenly appears for very high frequencies

{ BlitB3Saw.ar(MouseX.kr(10,10000,'exponential'),MouseY.kr(0.01,0.99)) }.play;

//comparison

{ Saw.ar(1000) }.play;

{ BlitB3Saw.ar(1000) }.play;

{ Mix(Saw.ar({rrand(10,1000)}!100,mul:0.01)) }.play;

//definitely more efficient second method

{ Mix(BlitB3Saw.ar({rrand(10,1000)}!100,mul:0.01)) }.play;

//see also comparison in BlitB3 help file